For:	FUJI Machine America Corporation		From:	Goda Advertising
	171 Corporate Woods Parkway			1603 Colonial Parkway
	Vernon Hills, IL  60061				Inverness IL 60067
	(847) 821-2432					(847) 776-9900 Ext. 124
	Fax: (847) 821-7815					Fax: (847) 776-9901
	Web site: www.fujimachine.com			Contact: Kim Maley
			E-mail: kmaley@goda.com

FOR IMMEDIATE RELEASE

FUJI’S NEW PBS-300TT TWIN TURRET CHUCKER MEETS DEMAND 
FOR HIGHLY PRODUCTIVE 4-AXIS ID AND OD DIAMETER CUTTING
 
Vernon Hills, IL – Now available from Fuji, the PBS-300TT Twin Turret Chucker performs medium to high volume production with short cycle times. In fact, featuring 4-axis simultaneous ID/OD diameter rough and finish turning, the PBS-300TT provides about a 38% reduction in process cycle time. The rigid box way construction of this chucker ensures superior spindle output. 
Equipped with Fuji’s own high-speed 3-axis dual hand gantry robot, the PBS-300TT provides work piece loading and unloading efficiency. Robot carrying capacity of this Fuji’s Chucker is 6.6 lbs. + 6.6 lbs., conveying diameters up to 7” inch X   4.7” length. The PBS-300TT comes with FUJI’s SP1 Max Robot Controller for faster and smoother simultaneous multi-axis movement to access the front, back, left and right of the traverse axis.
A Fanuc 320i-A CNC Control is standard with 5-place decimal positioning control (English); 4-place metric is also included. 
The PBS-300TT operates at a maximum spindle speed of 3,000 rpm and generates 20hp at the spindle motor. The turret head features a curvic coupling. For improved chip flow, the machining position of the PBS-300TT is located directly above a large chip receptacle at the bottom of the machine. Chips drop straight down from the cutting zone onto the Fuji built chip conveyor.
The PBS-300TT is suitable for machining flanges, hubs, gear blanks, inner rings, outer rings and more. 
The compact footprint 4’11” W x 6’7” D x 10’ H of the PBS-300TT allows for easy integration into most shop environments.
FUJI turns the machining of a part into process perfection. When you contact FUJI, the part you will be machining is analyzed by engineers with vast experience in process and manufacturing engineering. With the largest install base at the major automotive manufacturers, FUJI engineers apply their experience with the FUJI machines that are built for automation from the ground up. These highly accurate machines employ built-in robotic automation, in-process auto gauging for quality control, and are engineered with the finest FUJI custom workholding, all from one source. This allows FUJI engineers to guarantee takt time, cycle time and CPK with turnkey and run-off solutions that are built for lean manufacturing. Using less manpower and more automation, FUJI machines produce the highest quality parts most efficiently and reliably. FUJI solutions are supported by factory-trained American engineers 24/7.
     For more information, log on to www.fujimachine.com or contact FUJI Machine America Corporation, 171 Corporate Woods Parkway, Vernon Hills, IL 60061, Phone: 847-821-2432, Fax: 847-821-7815, email: info@fujimachine.com.

-30-